\*\*\*DENOTES: POR posted online

AU18/XXJUN18/EMAIL TO SML/ROB/POR2/PIC IN FOLDER

Open frame ac-dc converter boosts input voltage

AMEOF5-BJZ 5W compact open frame ac-dc converter complements the current 90-528Vac ultra-wide input voltage range. Product’s open frame design has an operating temperature range of -40°C to +85°C and has full power output between -20°C and +55°C. The output voltage options are 3.3, 5, 9, 12, 15 and 24V for both the standard and the right-angled SIP version. Product provides low power consumption, high efficiency & reliability, 4000Vac isolation and continuous short circuit protection.

AIMTEC

www.aimtec.com/home

RSN